CHANGES.txt - Change History for MyForth

07May07rjn
==========
1. Cleaned up MyForth prior to a confidential transmission to Bill Kibler.
The zip file contains code for clients not meant for general distribution.

2. Eliminated the old ~ backup files, some obsolete directories and code.

3. Moved startup batch files, such as lcd.bat, from the root to the project
directories so that they didn't have to be re-created.


15Apr07rjn
==========
1. Deleted serial-linux.fs and serial-widows.fs from the MyForth directory.
These should be in the processor directories (e.g., \MyForth\120) because
of the typical setups for baud rate, com port, etc., which may change between
processors (baud rate) and projects (com port).  This ensures that the 
configuration is more useable at startup.  

2. Also added serial-linux com3.fs to the 120 directory to make it easier 
to change to com3 (SL 2102 USB evaluation board).  

3. Note: I had some problems executing the "d" command after downloading 
chip.hex to a new 120 board.  It turned out to be related to the USB Debug
Adapter -- all was ok after I disconnected its cable to the 120 board and 
recycling power.  Sometimes it is ok leaving it plugged in, sometimes not.  
This isn't a problem after first bootloading, but ...
I suspect it has to do with options to disconnect after the IDE terminates.
Although the USB Debug Adapter does not have a status light lit, it appears
to affect the JTAG interface.
